|  |  |  |  |
| --- | --- | --- | --- |
| **Quote Number** | **Project Name** | **Project Location** | **Date** |
| Q-J-24-6499-REV 0 | MIDDLEBURGH WELL HOUSE |  | 6/3/2024 |
| |  |  | | --- | --- | | **From:** | David Lavender | | **Cell:** | 518-369-0272 | | **Email:** | DLavender@kinsleypower.com | |  |  | |  |  | |  |  | | | | |

|  |  |
| --- | --- |
| **Qty** | **Bill of Material Summary** |
|  |  |
| 1 | **Kohler KG60 Generator**  **Output -** 62kW, 78kVA, 277/480 Volt, Three Phase, 94amps, 60 Hz  **Fuel Type** - Propane  **Enclosure –** Weather  **Warranty -** 1 Year Standard  **Estimated Leadtime -** 30 Weeks, ARO |
|  |  |
|  |  |
|  |  |
|  |  |
| 1 | **Distributor Start-Up**  Start-up Service with Connected Load Test & Batteries |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Spec/Notes:** |  | | | | |
| **Terms** | | **Retainage** | **F.O.B.** | **Mfg. Manuals** | |
| Net 30 or Prior to SU | | No Retainage Allowed | Source | 1 | |
| **OFFER TOTAL SELL PRICE: $24,450.00** | | | | |
|  | | | | |
| *Quote is valid for 30 days.*  *Kinsley Power Systems reserves the right to amend this price quote when equipment is released for production without penalty or charge due to unprecedented price fluctuations in raw materials and components.* | | | | |
| Price does not include state sales tax, or installation | | | | |
|  | | | | |

|  |  |  |
| --- | --- | --- |
|  | **Kohler Model: KG60**  This LP generator set equipped with a 4P8X alternator operating at 277/480 volts is rated for 62kW/78 kVA. Output amperage: 94 |  |

|  |  |  |
| --- | --- | --- |
|  | **Qty** | **Description** |
|  |  | KG60 Generator System |

|  |  |  |  |
| --- | --- | --- | --- |
|  | 1 | KG60 Generator Set | |
|  |  | **Includes the following:** | |
|  |  | Literature Languages | English |
|  |  | Approvals and Listings | UL2200 Listing/cUL Genset List |
|  |  | Engine | Single Fuel, LP, Stdby |
|  |  | Nameplate Rating | Standby 130C Rise |
|  |  | Voltage | 60Hz, 277/480V, Wye, 3Ph, 4W |
|  |  | Alternator | 4P8X |
|  |  | Cooling System | Unit Mounted Radiator, 50C |
|  |  | Skid and mounting | Skid, 41" |
|  |  | Air Intake | Standard Duty |
|  |  | Controller | APM402 |
|  |  | Enclosure Type | Weather |
|  |  | Enclosure Material | Steel |
|  |  | Starting Aids, Installed | 1500W,120V |
|  |  | Electrical Accy., Installed | Battery, 1/12V, Wet |
|  |  | Electrical Accy., Installed | Battery Charger, 6A |
|  |  | Electrical Accy., Installed | Run Relay |
|  |  | Rating, LCB 1 | 80% Rated |
|  |  | Amps, LCB 1 | 110 |
|  |  | Trip Type, LCB 1 | Thermal Magnetic |
|  |  | Interrupt Rating LCB 1 | 18kA at 480V |
|  |  | Miscellaneous Accy, Installed | Coolant in Genset |
|  |  | Warranty | Standard |
|  | 1 | Flexible Fuel Line (Nat/LP) UL | |

|  |  |
| --- | --- |
| **OFFER ACCEPTANCE** | |
| I hereby authorize Kinsley Power Systems, Inc. to use this form as a bona fide purchase order of the equipment shown on Proposal Number QUO-54609-Q8X7X which clearly establishes definite price and specifications of material ordered. The person signing is doing so according to the terms and conditions below. | |
|  | |
| |  |  |  |  | | --- | --- | --- | --- | | **Proposed By:** |  | **Accepted By:** |  | | Company: | Kinsley Power Systems, Inc. | Company: |  | | Signature: | David Lavender | Signature: |  | | Printed Name: | David Lavender | Printed Name: |  | | Title: | Sales Engineer | Title: |  | | Date: | 6/3/2024 | Date: |  | | |
| **TERMS & CONDITIONS:** |
| **Agreement subject to Terms and Conditions available at** <https://www.kinsley-group.com/generalterms/>**.** |
| |  |  | | --- | --- | | **INSTALLATION**  **(not included)** | Defined as to include but not limited to; rigging, wiring, plumbing, fuel or fuel for testing, unless noted.  All "**Shipped Loose**" items are to be installed by others; including enclosure hoods, stacks, stairs, silencers, etc. | | **ESTIMATED SHIPPING** | **Ship dates are best estimates only. Therefore, Kinsley Power Systems is not responsible for incidental or liquidated damages.** | | **TERMS** | Net 30 days from shipment date or prior to start-up whichever comes first; subject to credit approval. Orders greater than $500,000 will be subject to a payment schedule negotiated between Seller and Buyer. We reserve the right to charge 1.5% on accounts over 30 days past due. Our price does not include sales tax or installation. | | **CANCELLATION/BILLABLE DELAYS** | **If the manufacturer will allow order to be cancelled a re-stocking charge will apply. Orders placed on in-stock items which are not shipped or picked up after 15 days of order date will be returned to inventory for sale to others. Factory-ordered units shipped to a Kinsley facility for temporarily storage due to customer payment or jobsite readiness issues are subject to storage fees of 1% per month unless order is paid in full.** | | **CONTRACT CHANGES** | A mutually agreed to, signed change order is required for any contract changes. | | **RETAINAGE** | None | | **FREIGHT** | F.O.B. Factory, Freight Allowed; Tailgate Delivery, Off-loading by others. Shipping addresses must be deliverable by an LTL carrier. Ex: No dirt roads, steep or narrow driveways etc. Delivery truck must be able to turn around or back in safely. Please specify special delivery requirements. Unless otherwise specified, additional charges will apply. | | **MANUALS** | One set of manuals is included with each unit. Additional manuals can be ordered at additional cost. | | **WARRANTY** | Manufacturer's standard warranty terms and conditions apply. | | **START UP** | Start-up service is during normal business hours. After hours or weekend start up is available at an additional cost. Unless otherwise noted, all 3rd party testing such as NETA, Insulation Resistance, Ground Fault, Infrared Scanning, emissions testing, exhaust backpressure testing, etc. to be provided by others | |

**I acknowledge that I have read and agree to all the above Terms and Conditions: \_\_\_\_\_\_\_\_\_\_**

(Initial)